|  |  |
| --- | --- |
| Date:       | **Harness Specification Sheet**Customer Notes:       |
| Dealer Name:       | Customer Notes:       |
| Customer Name:       |
| Daytime Contact No:       |
| Email Address:       |
| Approval Type:   | Qty required:  | Colour:  |

|  |  |  |
| --- | --- | --- |
| Make of Vehicle:       | Type:       | Year:       |

|  |
| --- |
| **Shoulder strap measurements “A” should be taken with driver seated in vehicle with harness fastened tight.**TRS Technical Tip: Shoulder measurements “A” under 65cm TRS recommend a Sewn Bearing Point |
| Sewn Bearing Point **[ ]**  | Threaded Anchor Point with 3 Bar Slide **[ ]**  | **Shoulder Webbing Width:**FHR Specific 50mm **[ ]** 75mm **[ ]**  | **Length A:**      **cm**Measure distance “A” from centre of anchor mounting point to centre of adjuster |
|  |  |  |
| **Shoulder Adjuster (Mark appropriate box)**TRS Technical Tip: TRS Recommend the aluminium adjuster for fast and easy adjustment |
| **75mm Steel Adjuster [ ]**  | **75mm Aluminium Adjuster [ ]**  |
|  |  |

|  |
| --- |
| **Lap Straps - Measurements should be taken with the harness fastened tight and adjustment in midway position.**“B” is 65cm as standard from centre of anchor mounting to centre of release buckle.“C” is 12cm as standard from centre of mounting strap to centre of adjuster. |
| **Pull Up**(STD Direction) | **[ ]**  |  | **Length B:**(Overall Length)**Length C:**(Adjuster Length) |       **cm**      **cm** |
| **Pull Down**(Suited for tight cockpits i.e. Kit Car) | **[ ]**  |  | **Length B:**(Overall Length)**Length C:**(Adjuster Length) |       **cm**      **cm** |
| **Lap Adjuster (Mark appropriate box)**TRS Technical Tip: TRS Recommend the aluminium adjuster for fast and easy adjustment |
| **75mm Steel Adjuster [ ]**  | **75mm Aluminium Adjuster [ ]**  |
|  |  |

|  |
| --- |
| **Rotary Quick Release Buckle Only**Permanently fixed to Crotch Strap M10-0003 (Standard for a 5pt/6pt Saloon) |
|  |

|  |
| --- |
| **50mm** **Crutch Straps - Measurements should be taken with the driver seated in the vehicle.****2-point Crutch Moustache**“D” is 65cm as standard. |
| **Pull Down**  | **[ ]**  |  | **Length D:** |       **cm** |

|  |
| --- |
| **Sewn Anchorages - Mark appropriate boxes to identify requirements** |
| Sewn Snap Hook | Sewn 8mm Bolt in Plate | Sewn 9.5mm Bolt in Plate | Sewn 11mm Bolt in Plate | Sewn 13mm Bolt in Plate | Sewn 15mm Bolt in Plate | Sewn Flat Loop4cm is standard | Sewn Pinched Becket4cm is standard | Sewn Carabina |
|  |  |  |  |  |  |  |  |  |
|  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  |  | [ ]  | **FHR 50mm****Shoulder Straps** |
|  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  | [ ]  | **75mm****Shoulder Straps** |
| [ ]  | [ ]  | [ ]  |  |  | [ ]  | [ ]  |  | [ ]  | **75mm Lap Straps** |

|  |  |
| --- | --- |
| **Threaded Anchorages - Mark appropriate boxes to identify requirements** |  |
| Snap Hook + 3 Bar Slide | 13mm Bolt in Plate + 3 Bar Slide | Wrap Around | 8mm Bolt in Plates as Pinch Plates |  |
|  |  |  |  |  |
| [ ]  | [ ]  |  |  | **FHR 50mm****Shoulder Straps** |
| [ ]  | [ ]  | [ ]  |  | **75mm****Shoulder Straps** |
| [ ]  |  | [ ]  |  | **75mm Lap** **Straps** |
| [ ]  | [ ]  | [ ]  | [ ]  | **50mm Crutch Straps** |